(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A5")
  (title_block
    (title "Siedle NG 402-01")
    (date "2022-03-27")
    (rev "1")
    (company "Julian Heinzel")
    (comment 1 "Creative Commons Attribution 4.0 International (or later)")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user "Nutzer.1")
    (51 "User.2" user "Nutzer.2")
    (52 "User.3" user "Nutzer.3")
    (53 "User.4" user "Nutzer.4")
    (54 "User.5" user "Nutzer.5")
    (55 "User.6" user "Nutzer.6")
    (56 "User.7" user "Nutzer.7")
    (57 "User.8" user "Nutzer.8")
    (58 "User.9" user "Nutzer.9")
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (gr_line (start 135.5 50) (end 135.5 72) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 135.5 72) (end 127.5 72) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 124.5 75) (mid 125.37868 72.87868) (end 127.5 72) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 124.5 86) (end 124.5 75) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 50 50) (end 50 86) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 50 86) (end 124.5 86) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 50 50) (end 135.5 50) (layer "Edge.Cuts") (width 0.1))
)
